*************************** START ****************************

Chip: ESP32S3
Download mode: uart
Start time: 20260423-11:37
Connect baud: 115200
Com:COM18
connecting...
manufacturer_id: 0x5e
device_id: 0x4018
fs:0x100200
address/file: 0 G:\3.5inch_ESP32-S3-资料包\8-快速使用_Quick_Start\Flash_download\flash_download_tool\dl_temp\bin_tmp\downloadPanel1\2.8inch_ESP32-S3_Production_Test(1).bin

Wrote 2118768 bytes (1387920 compressed) at 0x00000000 in 14.4 seconds (effective 1177.3 kbit/s)...

File: G:\3.5inch_ESP32-S3-资料包\8-快速使用_Quick_Start\Flash_download\flash_download_tool\dl_temp\bin_tmp\downloadPanel1\2.8inch_ESP32-S3_Production_Test(1).bin
File  md5: ae9ac08244a021b99a6da0f865e2f608
Flash md5: ae9ac08244a021b99a6da0f865e2f608
Hash of data verified.

Leaving...

com closed
Total use time: 20 s

Download result: PASS

*************************** END ****************************



