CHANGE HISTORY:

Will Never Happen:
    R61520 vert scroll is not possible
	ST7781 vert scroll is not implemented
    ILI9320, 9325, ... can never vert scroll sub-window 

To Be Fixed:
	GLUE Demo seems ok now

v2.9: posted 05 May 2016
    MCUFRIEND_kbv.cpp:  
			Added pushCommand() method   to send block of 8-bit SRAM data to MIPI controller
			SSD1963 fixed aspects.
			Added ILI9302
			Added ILI9338
			Added R61520
			ILI9327 defaults to shifted band in REV modes.  #define OFFSET_9327			
			Conditional S6D0139.    #define SUPPORT_0139 Untested
			Conditional HX8347-A.   #define SUPPORT_8347A Untested
			Conditional HX8347-I.   #define SUPPORT_8347D
			Conditional SSD1289.    #define SUPPORT_1289
	UTFTGLUE.h:
	        implement drawBitmap() method. (no rotations)
    LCD_ID_readreg.ino:
	        write(0xB0, 0x00) after hardware Reset to read manufacturer locations.
			added some extra registers.
v2.8: posted 26 February 2016
    MCUFRIEND_kbv.cpp:  LANDSCAPE is now 90 degrees instead of 270 degrees
	                methods branch on MIPI / 9320 style
			Added SPFD5408
			Added R61505W     Untested
			Added HX8347-A    Untested
		        Added SSD1963     Untested
    graphictest_kbv.ino: smaller buffer for Software Scroll.  Just fits in Uno Flash
    TouchScreen_Calibr_kbv: wait for consistent Touch
    LCD_ID_readreg:     Added some more registers
	
v2.7: posted ........ NOT YET
v2.6: posted ........ NOT YET
    MCUFRIEND_kbv.cpp:  
                        Added R65105V
						
v2.5: posted 11 January 2016
    MCUFRIEND_kbv.cpp:  
                        Added ST7789V
                        Added RM68090
                        Added ILI9481
                        Added pushColors() from Flash
                        Improved downward Vertical Scroll.   API is changed.
                        ILI9327 should work in all aspects. vertical scroll in PORT/LAND_REV
                        S6D0154 should vertical scroll a subwindow
                                            
    graphictest_kbv.ino: smooth colour gradation on rounded rectangle tests on bigger displays
                        added colour grading range.
                        added vertical scroll down
                        improve messages
    
    graphictest_slim.ino: reduced-fat version of graphictest_kbv.ino
    testcard_kbv.ino:   drawn version of common BMP photo.
	scroll_kbv.ino:     changed vertScroll() call for new API    
    
    UTFTGLUE.h:         improve calculate width and height of rectangles from coordinates.
    
v2.4: posted 10 December 2015
    MCUFRIEND_kbv.cpp:  LGDP4535 initialisation table fixed - UNTESTED 
    
v2.3: posted 8 December 2015
    MCUFRIEND_kbv.cpp:  added S6D0139 UNTESTED
                        detect EXTC=0 ILI9341 shield from DX with ID == 0x0000.   drive in RGB mode
                        ILI9327 should Vertical Scroll now. UNTESTED
    UTFTGLUE.h:         extra print(const char*) method to avoid warning messages
                        
    graphictest_kbv.ino: software scroll a smaller block at top of screen
    GLUE_Demo_320x240:  removed unnecessary "include Adafruit_TFTLCD.h" 
    aspect_kbv.ino:     invert display when in different aspects 
    readpixel_kbv.ino:  support smaller geometries
    LCD_ID_readreg.ino: report some more regs
    TouchScreen_Calibr_kbv: for resistive Touch screens like on Mcufriend shields
    UTouch_Calibr_kbv:  can use UTouch.h library for hardware Touch Controllers (and UTFT)

v2.2: posted 15 November 2015
    MCUFRIEND_kbv.cpp:  changed readGRAM() for ILI9327, ILI9486,
                        added REV_SCREEN flag to _lcd_capable
                        implement invertDisplay()
                        added LGDP4535
                        ILI9327: set Partial Area to 0, 399                        
    MCUFRIEND_kbv.h:    USE_GFX_KBV default argument: println(char *s="")
    MCUFRIEND_shield.h: regular Uno shield drivers for Uno, Mega, Leonardo, Due, Zero
    MCUFRIEND_special.h:  experimental drivers
    UTFTGLUE.h:         identity kludges for non-UNO shields
    LCD_ID_readreg.ino: report reg(0x09)

v2.1: posted 9 November 2015
    MCUFRIEND_kbv.cpp:  return 0x9327 / 0x9481 in readID()
    MCUFRIEND_shield.h: increase low pulse width in RD_STROBE
    EXAMPLES/:          add scroll_kbv.ino sketch
                        edit readpixel_kbv_ino,  aspect_kbv.ino

v2.0: posted 8 November 2015
    Massive changes from v1.0


