#

##

##

##

    礦ision Build Log
    Tool Versions:
    IDE-Version: μVision V5.11.2.0
    Copyright (C) 2014 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: IBM Microsoft, Microsoft, LIC=TA3Z9-4TC1X-22VL4-FRF0J-D7AGZ-Q8RWL

    Tool Versions:
    Toolchain:       MDK-ARM Professional  Version: 5.10.0.0
    Toolchain Path:  d:\Keil_v5\ARM\ARMCC\bin\
    C Compiler:      Armcc.exe V5.04 update 1 (build 49)
    Assembler:       Armasm.exe V5.04 update 1 (build 49)
    Linker/Locator:  ArmLink.exe V5.04 update 1 (build 49)
    Library Manager: ArmAr.exe V5.04 update 1 (build 49)
    Hex Converter:   FromElf.exe V5.04 update 1 (build 49)
    CPU DLL:         SARMCM3.DLL V5.10.0.0
    Dialog DLL:      DCM.DLL V1.10.0.0
        Target DLL: Segger\JL2CM3.dll
    Dialog DLL:      TCM.DLL V1.14.1.0

    Project:
    E:\project\3.2inch\QDtech_3.2inch_ILI9341_SPI_V1.0\2-STM32测试程序\STM32_Demo_STM32F103RCT6_Software_SPI\USER\TOUCH.uvproj
    Project File Date:  07/06/2018

    Output:
    Build target 'Target 1'
    compiling main.c...
    compiling test.c...
    compiling GUI.c...
    compiling lcd.c...
    compiling touch.c...
    linking...
    Program Size: Code=18566 RO-data=8854 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\TOUCH.axf"
    Set JLink Project File to "E:\project\3.2inch\QDtech_3.2inch_ILI9341_SPI_V1.0\2-STM32测试程序\STM32_Demo_STM32F103RCT6_Software_SPI\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RC" selected (256 KB flash, 48 KB RAM).

    JLink info:
    ------------
    DLL: V4.80g, compiled Feb 13 2014 20:50:02
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 308621590
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RC
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...

et info: ------------ Device: STM32F103RC VTarget = 3.300V State of Pins: TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1 Hardware-Breakpoints: 6 Software-Breakpoints: 8192 Watchpoints: 4 JTAG speed: 2000 kHz Erase Done. Programming Done. Verify OK. Application running ...