# Waveshare ESP32-S3-Touch-AMOLED-1.75


[ESP32-S3-Touch-AMOLED-1.75](https://www.waveshare.com/esp32-s3-touch-amoled-1.75.htm) ESP32-S3-Touch-AMOLED-1.75 is a high performance, highly integrated microcontroller development board designed by Waveshare.\
In the smaller form, the 1.75-inch capacitive HD AMOLED screen, highly integrated power management chip, six-axis sensor (three-axis accelerometer and three-axis gyroscope), RTC, low-power audio codec chip and echo cancellation circuit are mounted on the board, which is convenient for development and embedding into the product.


## images

| [ESP32-S3-Touch-AMOLED-1.75](https://www.waveshare.com/esp32-s3-touch-amoled-1.75.htm)                                                                                                                                                                                           |
|-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------|
| <img style="width: 150px; height: auto; display: block; margin: 0 auto;" src= "https://www.waveshare.com/media/catalog/product/cache/1/image/800x800/9df78eab33525d08d6e5fb8d27136e95/e/s/esp32-s3-touch-amoled-1.75-1.jpg"> |
| <img style="width: 150px; height: auto; display: block; margin: 0 auto;" src= "https://www.waveshare.com/media/catalog/product/cache/1/image/560x560/9df78eab33525d08d6e5fb8d27136e95/e/s/esp32-s3-touch-amoled-1.75-b-3.jpg"> |
| <img style="width: 150px; height: auto; display: block; margin: 0 auto;" src= "https://www.waveshare.com/media/catalog/product/cache/1/image/560x560/9df78eab33525d08d6e5fb8d27136e95/e/s/esp32-s3-touch-amoled-1.75-b-1.jpg"> |

